### Installing a Windows NT 4.0 Driver from Diskette

This topic describes how to install a Digi driver from diskettes.

#### Procedure

1. From the Windows NT Control Panel, select the Network icon.

2. Select the Adapter tab, then click Add. The Select Network Adapter dialog will be displayed. Click Have Disk. You will now be asked to enter the path of the driver files. For example: a:\i386 if you are installing from a floppy to an Intel system, or a:\alpha if you are installing from a floppy to an Alpha system.

3. From the displayed pick list, select the adapter you wish to configure.

4. If the adapter is an ISA adapter, enter the I/O base port address and the Memory base address. You will also see a pictorial representation of the DIP switches on the end of the adapter; the graphic shows the correct switch setting for the selected I/O base port address (the memory base address for AccelePort adapters is set by the device driver).

5. For C/X, EPC/X, and Xem systems, you will now be presented with dialogs for adding concentrators and PORTS and/or Modem/Xem modules to the configuration. These dialogs are documented in help screens.

6. Once the adapter, concentrators and modules have been configured, you will see a "tree" of the system. To configure the adapter, concentrators, modules or ports, select the desired item and click the Properties button.

7. Once all parameters have been set as desired, click "OK".

8. If you are installing multiple PCI adapters, install the next adapter and repeat the above steps.

Copyright © 1999, Digi International. All rights reserved.