### NetWare Xe Error Messages and Solutions

#### Load Command Errors

The following error messages may occur while the driver is parsing the parameters.

*Usage Error: AIODGXI port=XXXX mem=XXXXX [name=bname].

| This error will appear if you load the driver with no parameters on ISA bus computers.

*Usage Error: First parameter not 'port='.

| The driver expects the first parameter to be port=xxx, but this was not the case.

*Error: Invalid Port Address 0x310.

| This message indicates that an invalid port address was speci-fied.

*Error: Port Address 0x320 is already supported.

| This message indicates that the driver is already supporting an adapter at this port address.

*Usage Error: Second parameter not 'mem='

| The driver expects the second parameter to be mem=xxxxx, but this was not the case.

*Error: Invalid Memory Address 0xF0000.

| This message indicates that an invalid memory address was specified.

#### Adapter Errors

The following error messages may occur while the driver is performing some initial tests on the adapter.

Adapter 4: Port 220 Mem D0000 Port 220 not found.

| This message indicates that the driver could not find an adapter with port 220h. Check to insure that you have specified the cor-rect I/O port or that you have properly configured the adapter's port ad-dress.

Adapter 4: Port 220 Mem D0000 Hardware Reset Fails.

| This message indicates that the driver could not place the adapter into a reset state. This is most likely the result of an I/O port ad-dress conflict or a faulty adapter. Be sure that there are no other I/O ports in your system at the indi-cated I/O port address.

Adapter 4: Port 220 Mem D0000 Memory not found error x.

| This message indicates that the driver could not find the adapter's memory. x indicates the num-ber of memory errors found in a 256 byte block.

Adapter 4: Port 220 Mem D0000 Memory error x.

| This message indicates that the driver has found the adapter's mem-ory, but it appears to be faulty. x indicates the number of errors found in a 256 byte block.

#### Initialization errors

The following messages may occur during the driver's attempt to initial-ize the adapter.

Adapter 4: Port 220 Mem D0000 BIOS fails initialization.

| This message indicates that the adapter's on-board BIOS did not initialize properly.

Adapter 4: Port 220 Mem D0000 BIOS passes init but reports 0 ports.

| This message indicates that the BIOS initialized successfully, but could not find any of the asynchro-nous channels.

Adapter 4: Port 220 Mem D0000 NMI Fails during FEPOS code move.

| This message indicates a failure during transfer of the on-board operating system code.

Adapter 4: Port 220 Mem D0000 NMI Fails during FEPOS execution.

| This message indicates a failure during startup of the on-board operating system.

Adapter 4: Port 220 Mem D0000 FEPOS Fails Initialization.

| This message indicates that the on-board operating system did not initialize successfully.

Adapter 4: Port 220 Mem D0000 Command failure during Initialization.

| This message indicates that the on-board operating system en-countered a failure during in-itiali-zation of the asynchro-nous chan-nels.

Copyright © 1999, Digi International. All rights reserved.