### Installing ISA Drivers for Windows 95/98 from Diskette

#### Prerequisite

To install software on a computer that doesn't have a CD drive, you must create an installation diskette from the CD.

For instructions on creating installation diskettes, see:

Creating Installation and Diagnostic Diskettes

#### Procedure

1. From the Windows Control Panel, start the Add New Hardware wizard.

2. Click Next to begin installing new hardware.

3. You will be asked: Do you want Windows to search for your new hardware? Select No, then click on Next.

4. Highlight the Other Devices hardware type, then click on Next (on subsequent installs you will be able to select AccelePort Adapter for the hardware type).

5. Click on Have Disk.

6. On the Install from Disk applet, enter A: (for drive A) when asked for the location of the Digi Windows 95 driver files, then click on OK.

7. A list of Digi adapter choices will appear. Select your adapter from the list and click on Next.

8. Write down or print the displayed list of hardware settings.

9. Click Next. The driver files will be copied to your system.

10. The Ports Configuration property page will be displayed for you to view and edit the assigned port names. For an Xem adapter, you will need to configure the PORTS modules that are connected to your adapter. On-line help is available for more information. When you are finished, click OK.

11. Click Finish.

12. A System Settings Change applet will ask whether you want to shut down your computer now. Click on Yes.

13. Turn off your computer and then change the adapter to match the resource settings you gathered in step 8.

14. Restart the computer. Digi's driver will load.

Copyright © 1999, Digi International. All rights reserved.