### Windows NT RAS Setup Overview

This procedure enables AccelePort RAS to handle modem calls.

#### Overview of Setup Steps

1. Install the adapter. See the appropriate hardware installation card for instructions.

2. Install the driver and configure for BRI. See Installing a Windows NT 4.0 Driver from CD for installation instructions; see the Digi Configuration Wizard and the online help for aid in configuring BRI.

3. Configure RAS ports. See Configuring RAS Ports on Windows NT 4.0. This includes the following:

   - Configuring modems as RAS ports

   - Configuring the network protocols to use on each modem

4. Configure RAS permission levels. See Configuring RAS Permissions on Windows NT 4.0.

5. If you want to enable outbound calling, configure Dial-Up Networking. See Configuring Dial-Up Networking Connections.

Copyright © 1999, Digi International. All rights reserved.