### Installing NetWare Driver Files at the Server Console

#### Prerequisites

- If you have a CD-ROM drive on your server, you can install the driver files for your AccelePort product directly from the CD.
  If you don't have a CD-ROM drive, you can still install at your server, but you must first make an installation diskette on a Windows or UNIX machine equipped with a CD-ROM drive. See:
  Creating Installation and Diagnostic Diskettes

- If you plan to use the CD, you need to know whether you have a DOS-mounted or a Novell-mounted CD-ROM drive. If it is DOS-mounted, the CD-ROM drive is accessible to DOS applications and NetWare applications without mounting.
  If your CD-ROM drive is Novell-mounted, you must be sure that all of the Novell CD-ROM device drivers are loaded, insert the CD, and enter the following command to mount it before you begin your installation:
  cd mount digi_cd

#### Procedure

1. At the system command prompt, type the following:
   load install
   A Novell menu will be displayed.

2. Choose Product Options, and then choose Install a Product Not Listed from the next menu that displays.

3. Choose a source directory from which the drivers will be copied.
   Press <Enter> if you are installing from a diskette.
   If installing from CD, press <F3>, then specify the path to the CD-ROM drive, as shown below:

   Dos Mounted | Novell-Mounted
   <Drive>:\Novell\directory | digi_cd:\Novell\directory

   where <Drive> is the drive letter of the CD device under DOS, and directory is the directory containing the driver files for your AccelePort adapter (see table):

   Directory | Product Family
   RAS | AccelePort RAS Family
   Xr | AccelePort Xr Family
   Xe | AccelePort Xe Family
   Xem | AccelePort Xem System
   CXP | AccelePort PCI C/X System
   CX | AccelePort ISA C/X System
   EPC | AccelePort EPC/X System

4. Choose Install Product from the menu.

5. At the prompt, choose the server on which you want driver files installed.

6. At the Start installation? prompt, choose Yes.

7. When the installation is complete, exit the installation and then bring down and restart the server.

Copyright © 1999, Digi International. All rights reserved.