### Configuring Client-to-Server Modems

This topic describes how to configure a Digi adapter for 56 Kbps modems.

#### Prerequisites

This topic assumes that you have loaded niascfg or nwconn.

#### Procedure

1. Access the Remote Access Options menu. Here are path to the menu:

   - For NIAS: Configure NIAS > Remote Access.

   - For Connect: When you load nwconn, the menu appears.

2. Select Set Up ... .

3. Select Add a Serial Adapter Board.

4. Configure ports for modems. Here are some tips:

   - Do not auto-detect a modem type. It is much faster to do this manually.

   - Specify the same modem type for all ports.

   - Select the Rockwell Compatible 56K modem from the Modem Name list.

Copyright © 1999, Digi International. All rights reserved.