### Installing Digi PCI Adapters

Follow the instructions below.

CAUTION! To guard against damaging the Digi adapter by electrostatic discharge, do not remove the adapter from its protective packaging until you have grounded yourself to the computer chassis (see step 4, below).

1. Unplug power from the computer.

2. Remove the computer's cover.

3. Locate an available PCI slot in your computer and remove the slot plate.

4. Put on an elecrostatic discharge wrist strap and attach it to the computer's chassis.

5. Remove the Digi adapter from its protective packaging.

6. Record the serial number of the adapter in case you need to contact Technical Support. The serial number label has the general form: "S/N (S) XXX XXXXX".

7. Insert the adapter into the slot and screw the endplate to the computer chassis. The endplate must be screwed into the computer chassis to remain in compliance with Part 15 of FCC rules.

8. Replace the computer's cover.

Copyright © 1999, Digi International. All rights reserved.