### Installing AccelePort ISA Adapters

Follow the instructions below.

CAUTION! Do not remove the AccelePort adapter from its protective sleeve until you have grounded yourself to the computer chassis (see step 4, below).

1. Unplug power from the computer.

2. Remove the computer's cover.

3. Locate an available ISA slot in your computer and remove the slot plate.

4. Put on an elecrostatic discharge wrist strap and attach it to the computer's chassis.

5. Remove the AccelePort adapter from its anti-static sleeve.

6. Record the serial number of the adapter in case you need to contact Technical Support. The serial number label has the general form: "S/N (S) XXX XXXXX"

7. Set the adapter's DIP switches for the desired I/O address range (click the applicable link below to see a table of switch settings):

   - DIP Switch Settings for AccelePort Xr ISA Adapters

   - DIP Switch Settings for AccelePort Xe ISA Adapters

   - DIP Switch Settings for AccelePort C/X ISA Adapters

   - DIP Switch Settings for AccelePort EPC/X ISA Adapters

   - DIP Switch Settings for AccelePort Xem ISA Adapters

8. Insert the adapter into the slot and screw the endplate to the computer chassis. The endplate must be screwed into the computer chassis to remain in compliance with Part 15 of FCC rules.

9. Replace the computer's cover.

Copyright © 1999, Digi International. All rights reserved.