### Busying Out a Modem Channel

This topic describes how to busy out a modem channel, which is the means by which you disable a channel. Note: Busy out will terminate an active call.

1. Access the busy out function from one of the following:

   Adapter | Screen
   --- | ---
   DataFire RAS PT1 or PT2 | Line Summary Screen
   Acceleport RAS A | Modem Summary Screen

2. Click the Busy Out label associated with the channel you want to busy out.

3. Choose to Delay Busy Out until the channel is free or Busy Out, which means busy out the channel immediately.

4. Click OK.

Copyright © 1999, Digi International. All rights reserved.