### AccelePort RAS Setup Overview in SCO UnixWare

Here are the steps you perform to set up an AccelePort RAS adapter on SCO UnixWare.

#### Overview of Setup Steps

1. Install the adapter. See the appropriate hardware installation card for more information.

2. Install the SCO UnixWare driver. See Installing a SCO UnixWare Driver from CD.

3. Add the AccelePort RAS adapter to the WAN device list. See Adding a WAN Device.

4. Configure serial ports. See Configuring Serial Ports.

5. Configure PPP parameters with netcfg. See the SCO documentation for more information.

Copyright © 1999, Digi International. All rights reserved.