### EPC/CON-16 Concentrator Specifications

Power Requirements
+5 volts +/- 5% | 0.760 amps typical
+12 volts +/- 5% | 0.180 amps typical
-12 volts +/- 5% | 0.050 amps typical
Environmental
Ambient temperature | 5 to 50 degrees C
Relative humidity | 20% to 80%
Serial Interface Surge Suppression
Threshold voltage: |
(EIA-232) | 13 volts
(EIA-422) | 13 volts (input signals)
5 volts (output signals)
Response time | < 10 nS
Mechanical
| RJ-45 Model | DB-25 Model
Length | 12 inches | 12 inches
Width | 7 inches | 7 inches
Height | 2.25 inches | 4.2 inches
Weight | 2.25 pounds | 4.1 pounds

Copyright © 1999, Digi International. All rights reserved.