### V.35 Synchronous Cable Wiring - Winchester Connectors

V.35 wiring allows concentrators to be installed in remote locations and connected to the host adapter via V.35 DSUs/CSUs, frame relay adapters, fractional T1s or ISDN terminal adapters.

#### Host Adapter to Local V.35 Device

C/X or EPC/X Host Adapter (HD-15 Male) |  | Local V.35 Device (V.35 Male)
--- | --- | ---
Signal | Pin | Pin | Signal
RxD- | 1 | Connected to | R | RxD-A
RxD+ | 2 | Connected to | T | RxD-B
RxC- | 4 | Connected to | V | SCR-A
RxC+ | 5 | Connected to | X | SCR-B
TxD- | 6 | Connected to | P | TxD-A
TxD+ | 7 | Connected to | S | TxD-B
TxC- | 9 | Connected to | Y | SCT-A
TxC+ | 10 | Connected to | AA | SCT-B
GND | 12 | Connected (via shield) to | B | GND
Jumpered at V.35 End | C, D | RTS, CTS

#### Modem to Concentrator

Remote V.35 Device (V.35 Male) |  | Concentrator "Host Adapter" Port (HD-15 Female)
--- | --- | ---
Signal | Pin | Pin | Signal
RxD-A | R | Connected to | 6 | RxD-
RxD-B | T | Connected to | 7 | RxD+
SCR-A | V | Connected to | 9 | RxC-
SCR-B | X | Connected to | 10 | RxC+
TxD-A | P | Connected to | 1 | TxD-
TxD-B | S | Connected to | 2 | TxD+
SCT-A | Y | Connected to | 4 | TxC-
SCT-B | AA | Connected to | 5 | TxC+
GND | B | Connected (via shield) to | 12 | GND
RTS, CTS | C, D | Jumpered at V.35 End

Copyright © 1999, Digi International. All rights reserved.