### Configuring a Line: PPP WAN Calls

Use this procedure to configure PPP WAN calls.

#### Procedure

1. From the Internetworking Configuration menu, choose WAN Call Directory.

   The Configured WAN Call Destination screen appears.

2. Press the INSERT key.

3. Choose PPP Routing as the Supported Wide Area Medium.

   The PPP Call Destination Configuration screen appears.

4. Supply configuration information as required. You must specify a network interface in the Interface Name field and a telephone number.