### EPC/X Error Messages and Solutions

#### Installation Errors

If there is a problem with the installation, one or more of the following error messages may appear after you load the driver.

`*Error: Error Registering rfc-1406 for SNMP.`

> A problem was encountered while attempting to register the standard dsx1 MIB. Non fatal error.

`*Error: Error Registering DigiT1E1 MIB for SNMP.`

> The Digi specific MIB could not be registered. Management of this device with Quick Manager will not be possible. Non fatal error.

`*Error: Error Registering rfc-1659 for SNMP.`

> A problem was encountered while attempting to register the standard EIA-232 MIB. Non fatal error.

`*Error: Driver Already Loaded.`

> This message will appear if the driver is presently loaded. To reload the driver you must first unload the present memory copy of the driver by entering unload aiodgepc at the server console. Then you may reload the driver.

`*Error: Driver Configured for 0 adapters. Configure Driver with AIOEPCFG.NLM.`

> This message indicates that the driver is configured for 0 adapters. You must load aioepcfg to configure the driver to support at least one adapter.

`*Error: AllocateIOResourceTag failed.
*Error: Allocate Resource Tag failed.
*Error: AllocateAESResourceTag failed.
*Error: Allocation of PortConfig memory failed.
*Error: Allocation of PortStats memory failed.`

> These messages indicate that the driver encountered difficulties while trying to obtain resources from AIO. This usually indicates that the system is out of resources. Unload any unnecessary NLMs and reload the driver.

`*Error: AIORegisterDriverA failed (code=xx).`

> This message indicates that another driver has already registered the EPC/X hardware type (possibly illegally). Unload other AIO drivers and reload the EPC/X AIO driver.

`*Error: No PCI BIOS entry point found.`

> This message indicates that a PCI host adapter was configured, but the driver cannot locate the PCI BIOS.

`Adapter 0 : Port 208, Mem D0000 - Port 208 not found.`

> This message indicates that the driver could not find an adapter with port 208h. Check to insure that you have specified the correct I/O port or that you have properly configured the adapter's port address.

`Adapter 0 : Port 208, Mem D0000 - Hardware Reset fails.`

> This message indicates that the driver could not place the adapter into a reset state. This is most likely the result of an I/O port address conflict or a faulty adapter. Be sure that there are no other I/O ports in your system at the indicated I/O port address.

`Adapter 0 : Port 208, Mem D0000 - AIORegisterBoard failed (code=xx).`

> This message indicates that an error occurred while trying to register the adapter with AIO. This failure is usually the result of no system resources, or a duplicate adapter number. Check the driver configuration for duplicate adapter numbers. If none exist, unload unnecessary NLMs to free system resources.

`Adapter 0 : Port 208, Mem D0000 - Failed Hardware Registration.`

> This message indicates that an error occurred while trying to register the adapter's specific hardware addresses with AIO.

#### Resource Conflict Errors

The following error messages are usually the result of memory and/or I/O address conflicts with other devices within your system. Insure that no such conflicts exist. If errors persist, your adapter may be defective.

`Adapter 0 : Port 208, Mem D0000 - Memory not found error x.`

> This message indicates that the driver could not find the adapter's memory. x indicates the number of memory errors found in a 256 byte block.

`Adapter 0 : Port 208, Mem D0000 - Memory error x.`

> This message indicates that the driver has found the adapter's memory, but it appears to be faulty. x indicates the number of errors found in a 256 byte block.

`Adapter 0 : Port 208, Mem D0000 - Memory fails disable x.`

> This message indicates that the adapter's memory could not be disabled.

`Adapter 0 : Port 208, Mem D0000 - Unable to load BIOS file (\SYSTEM\DGEPCXB.BIN).`

> This message indicates that the specified BIOS file was not able to load properly.

`Adapter 0 : Port 208, Mem D0000 - Unable to load BIOS file (\SYSTEM\DGEPCXPB.BIN).`

> This message indicates that the specified BIOS file was not able to load properly.

`Adapter 0 : Port 208, Mem D0000 - BIOS fails initialization.`

> This message indicates that the adapter's on-board BIOS did not initialize properly.

`Adapter 0 : Port 208, Mem D0000 - NMI Fails during FEPOS execution.`

> This message indicates a failure during transfer of the on-board operating system code.

`Adapter 0 : Port 208, Mem D0000 - Unable to load FEPOS file (\SYSTEM\DGEPCXF.BIN).`

> This message indicates that the specified FEP/OS file was not able to load properly.

`Adapter 0 : Port 208, Mem D0000 - Unable to load FEPOS file (\SYSTEM\DGEPCXPF.BIN).`

> This message indicates that the specified FEP/OS file was not able to load properly.

`Adapter 0 : Port 208, Mem D0000 - FEPOS Fails Initialization.`

> This message indicates that the on-board operating system did not initialize successfully.

`Adapter 0 : Port 208, Mem D0000 - Command <x> failure during Initialization.`

> This message indicates that the on-board operating system encountered a failure during initialization of the asynchronous channels.

`Adapter 0 : Port 208, Mem D0000 - Memory Fails Window Test.`

> This message indicates that the adapter fails to window it's memory pages correctly.