### Configuring Modem Nationality: RAS Adapters

Use this step to configure the modem nationality for a Digi RAS modem.

Note: This step uses the device /dev/DIGIras/b00p00m as an example. Substitute your device name where necessary.

If necessary, configure the modem nationality by using a ras_config command at a Solaris root prompt:

> `ras_config -N nationality`

where `nationality` is the desired modem nationality. For detailed information on ras_config, enter the command without any options:

> `ras_config`

Note: The ras_config executable is in the directory /opt/DIGIras/bin. Add this path to the command if ras_config cannot be found on execution:

> `/opt/DIGIras/bin/ras_config`