### Configuring the EtherLite for RealPort

Use this process to install and configure the EtherLite Terminal Server on the RealPort.

1. Attach the EtherLite module to the network using only a 10Base-T cable. Do not plug in the power cable at this time.
2. Assign an IP address to the EtherLite module. Use one of the following methods:

> - Assigning an IP Address: Store IP
> - Assigning an IP Address: Digi's BootP
> - Assigning an IP Address (Temporary): Boot Console
> - Assigning an IP Address (Permanent): Boot Console.