### Digi EIA-485 Connector Wiring

Use the table below to see the pin assignments for the RJ-45 connector for EIA-485 multi-drop mode.

EtherLite 2 EIA-485 ports are wired for half duplex multiple-drop EIA-485 mode and have no termination installed.

Signal | Description | RJ-45 Pin
--- | --- | ---
- | no connection | 1
- | no connection | 2
- | no connection | 3
TxD(A)/RxD(A) | Transmitted/Received Data (A) | 4
TxD(B)/RxD(B) | Transmitted/Received Data (B) | 5
GND | Ground | 6
- | no connection | 7
- | no connection | 8