### Environmental Considerations and Cautions

The following is a list of environmental considerations that will ensure safe and efficient operation of your PortServer TS 8/16:

- Ensure that the PortServer has at least 12 inches (30 centimeters) of clearance on all sides to allow for proper ventilation. PortServers generate heat and requires adequate circulation to maintain proper operating temperatures. For the same reason, never cover or obstruct PortServer ventilation slots.
- Do not position the PortServer near high-powered radio transmitters or electrical equipment, such as electrical motors or air conditioners. Interference from electrical equipment can cause intermittent failures.
- Avoid exceeding the maximum cabling distances discussed in the Cable Guide section of this online manual. PortServer performance may be degraded.
- Do not install a PortServer in areas where condensation, water, or other liquids may be present. These may cause safety hazards and equipment failure.