### Master Setup Process

Use this process to install and configure the EtherLite Terminal Server on a Microsoft Windows NT system.

1. Attach the EtherLite module to the network using only a 10Base-T cable. Do not plug in the power cable at this time.
2. Assign the EtherLite module an IP address. See Assigning an IP Address: Store IP, Assigning an IP Address: Digi's BootP, Assigning an IP Address (Temporary): Boot Console, and Assigning an IP Address (Permanent): Boot Console.
3. Install the Windows NT driver. See Installing the Driver: CD or Installing the Driver: Downloaded.
4. Follow the prompts in the Configuration Wizard to configure the driver.