### EtherLite Specifications

WARNING: To prevent electric shock, do not remove the cover of an EtherLite module. There are no user-serviceable parts inside. Refer servicing to qualified personnel.

AC Power Requirements (maximum)
2-, 8-, and 16-port units | Two external power supplies available: 120 V AC, 60 Hz, 15VA (U.S., Canada) 100-240 V AC, 50-60 Hz, 15VA (universal)
32-port units | 100-240 V AC, 50-60 Hz, 25VA internal power supply
The recommended power cord for North American units is: UL Listed, CN, detachable type SJT or SVT, 3 conductor, 18 AWG, rated 125 V, 10 A.
Environmental
Ambient temperature | 50°F (10°C) to 104°F (40°C) for 2-, 8-, and 16-port units 50°F (10°C) to 95°F (35°C) for 32-port units
Relative humidity | 5% to 90% non-condensing
Altitude | 0 to 12,000 feet (0 to 3650 meters)
Serial Interface Surge Suppression
15 kilovolts per IEC 1000-4-2, Level 4
Mechanical
EL 2 models | Height: 1.2 inches (2.9 cm) Width: 3.8 inches (9.5 cm) Depth: 6.3 inches (16.0 cm) Weight: 0.5 lbs. (0.2 kg)
EL 8, EL 16, EL 160, EL 162 models | Height: 1.2 inches (2.9 cm) Width: 11.5 inches (29.3 cm) Depth: 5.4 inches (13.8 cm) Weight: 3.1 lbs. (1.4 kg)
EL 32 model | Height: 1.8 inches (4.5 cm) Width: 15.1 inches (38.4 cm) Depth: 7.6 inches (19.2 cm) Weight: 5.8 lbs. (2.6 kg)