### DataFire PTE Configuration Worksheet

#### Channelized T1, Long Haul (External T1)

Use the worksheet below to collect the information that may be required to complete the configuration of your DataFire PTE adapter within your operating system environment. Note that not all operating systems support all parameters.

The parameters on this page are for channelized T1 connected directly to an external T1 telephone line (Long Haul). If your adapter is connected to a PBX or similar in-house network, use the Short Haul worksheet. See Channelized T1, Short Haul (PBX or Other Internal Network).

Parameter | Value
--- | ---
Coding | [ ] B8ZS [ ] AMI
Framing | [ ] ESF [ ] D4
Long Haul Line Build Out (Level) | [ ] 0 dB [ ] 7.5 dB [ ] 15 dB [ ] 22.5 dB
Signaling | [ ] Ground Start [ ] Loop Start [ ] Immediate Start [ ] Wink Start -- Wink Digits (1-20): ________
Leased Time Slots | List which, if any, T1 time slots are leased:
Modem Nationality | Enter the country in which the PTE adapter will be installed: