### Configuring Dial-up Networking Connections

Use this procedure to configure Dial-up Networking connections for a Digi adapter.

#### Procedure

1. To access the Dial-up Networking utility, double-click My Computer and then Dial-up Networking.

2. Choose New.

3. Fill out configuration fields. Here are a few tips:

   - If you will use more than one telephone number to make the connection, do the following: (a) Fill in the telephone number (b) Choose the Alternate button, (c) Add numbers. (d) Choose OK when you are done.

   - In the Dial-up using field, specify the device that will be used for the connection.

   - If you want to configure a Multilink connection, do the following: (1) Choose Multiple Lines in the Dial-up using field. This entry will appear only if you have configured the connection in RAS for Multilink. (2) Choose Configure. (3) Check any channels that are to be part of the multilink connection.

   - When providing telephone numbers, remember the following: (a) You may have to include the number 9 or some other digit to get an outside line if your site uses a PBX or Centrex service. (b) For ISDN connections, do not use spaces, dashes, or commas in the telephone number. (c) If this is a long distance call, be sure the telephone number includes the number 1 and an area code.

   - When selecting ISDN Devices, select the line type ordered from your service provider.

4. Choose OK > Close.