### DataFire PTE Configuration Worksheet

#### ISDN E1 (Euro ISDN)

Use the worksheet below to collect the information that may be required to complete the configuration of your DataFire PTE adapter within your operating system environment. Note that not all operating systems support all parameters.

The parameters on this page are for ISDN E1 (Euro ISDN).

Parameter | Value
--- | ---
Line Type | E1
Framing | [ ] CEPT with CRC4 [ ] CEPT without CRC4
Coding | [ ] HDB3
Signaling | [ ] ETSI (Euro ISDN) [ ] None
Leased Time Slots | List which, if any, E1 time slots are leased:
Modem Nationality | Enter the country in which the PTE adapter will be operated: