### Adding a Digi Device with drpadmin

Use this procedure to create RealPort devices and start the RealPort daemons.

#### Procedure

1. Enter this command at a root prompt:

   /usr/sbin/drpadmin

2. Answer the prompts as appropriate.

   When Prompted to: | Action:
   --- | ---
   Select an option | Choose add.
   Enter the node name or IP address for this Digi device | If an IP address is used, make sure it is unique and does not conflict with any other network device. If a name is entered, the name must be registered in /etc/hosts or with an accessible nameserver.
   Enter the number of ports on the Digi device | Enter the number of ports for this Digi device. The installation will prompt to confirm this number. Note: If PORTS/Xem (EBI) modules will be attached to a PortServer II module, include these ports.
   Enter TTY device ID letter(s) | Enter one or two letters. These letters will be used to create the RealPort device names.
   Enter WAN speed if the connection between the Digi device and HP-UX system includes a WAN link slower than 1 MB | Enter the WAN speed if this is the case. Otherwise, choose Enter to continue.
   Confirm the configuration | Enter y to proceed or n to reenter the information.
   Select an option | Enter a to add another Digi device. Enter s to show configured Digi devices. Enter q to exit drpadmin.