### Channelized T1, Long Haul (External T1) Configuration Worksheet

Use the worksheet below to collect information that may be required to configure your DataFire PTE adapter in your operating system environment. Note that not all operating systems support all parameters.

The parameters on this page are for channelized T1 connected directly to an external T1 telephone line (Long Haul). If your adapter is connected to a PBX or similar in-house network, use the Short Haul worksheet. See Channelized T1, Short Haul (PBX or Other Internal Network).

Parameter | Value
--- | ---
Coding | [ ] B8ZS [ ] AMI
Framing | [ ] ESF [ ] D4
Long Haul Line Build Out (Level) | [ ] 0 dB [ ] 7.5 dB [ ] 15 dB [ ] 22.5 dB
EQ Gain Limit | [ ] High [ ] Low
Signaling | [ ] Ground Start [ ] Loop Start [ ] Immediate Start [ ] Wink Start -- Wink Digits (1-20): ________
Modem Nationality | Enter the country in which the PTE adapter will be installed: