### NetWare SYNC/570 Messages

After the system is rebooted if the driver does not initialize correctly, one of the following errors may be generated.

Message | Meaning
--- | ---
SYNC570: Fatal Error: Bad Channel/Line No Param. | An invalid channel number has been selected. An example would be trying to install channel 3 of a 2 port board. Check your board installation.
SYNC570: Fatal Error: The board cannot be found at IO port. | The board does not appear to be at that IO port. Please check your dipswitch settings.
SYNC570: Fatal Error: The Board is already initialized. | The driver has been called twice for the same board and port combination.
SYNC570: Fatal Error: The board memory address conflicts with system memory. | The SYNC/570 has been configured to be at an already allocated memory address. Please select another address.
SYNC570: Fatal Error: Board RAM failed the memory test. | A memory test has been executed on the SYNC/570 and this test has failed. Please check that there are no other adapters trying to use the selected memory address. This may indicated board failure.
SYNC570: Fatal Error: Channel already in use. | The selected channel has already been configured.
SYNC570: Fatal Error: Config File Not Found, Exiting | The name= parameter of the board load line has not been configured. Ensure that the driver load line (ex. "load SYNC/570.LAN port=120 mem=d8000 int=5 channel=1 name=fred") is the same as the configured board.
SYNC570: Fatal Error: Duplicate Memory Address. | Another adapter has already registered the configured SYNC/570 memory address. Please select another.
SYNC570: Fatal Error: Incorrect Major or Minor Version Numbers. | The Major and Minor version numbers of the TSM are invalid. Check your MPR 3.1 installation.
SYNC570: Fatal Error: The initialization parameter is out of range | An attempt was made to initialize the board with a parameter that was invalid.
SYNC570: Fatal Error: The initialization parameter is in error. | An attempt was made to initialize the board with an incorrect parameter.
SYNC570: Fatal Error: Invalid PCI Board Number or Board not usable. | An adapter board number was specified that exceeds the number of PCI adapters the driver has detected and determined to be usable.
SYNC570: Fatal Error: Maximum Number of Boards exceeded. | The driver supports up to four SYNC/570 adapters and that limit has been exceeded.
SYNC570: Fatal Error: Memory for the board could not be allocated. | The driver was unable to allocated memory for internal functions.
SYNC570: Fatal Error: No Port Addr Param. | The port address was not included on the command line. Make sure a port=xxx parameter is included on the load line.
SYNC570: Fatal Error: A null pointer was passed as an initialization parameter | The board was unable to be initialized.
SYNC570: Fatal Error: Parse Driver Parameter. | Invalid parameters were selected on the load line. Please check the load line for accuracy.
SYNC570: Fatal Error: SNMP Registration Failed. | The SNMP support was unable to register.
SYNC570: Fatal Error: TSM Port Registered Error. | Registration with the TSM failed. Ensure that the TSM has loaded. Check the board configuration.
SYNC570: Fatal Error: Unable to get memory. | The driver was unable to allocate memory for internal usage.
SYNC570: Fatal Error: Unable to get resource tag. | The driver attempted to allocate a resource tag and failed.
SYNC570: Fatal Error: Unable to get TSM entries. | The driver was unable to get the TSM entry points. Check board and port configuration along with MPR installation.
SYNC570: Fatal Error: Unable to Initialize Board. | Board initialization failed. Run diagnostics on the board.
SYNC570: Fatal Error: Unable to Initialize Port. | Port Initialization failed. Check for a bad board. Check port configuration in INETCFG.
SYNC570: Fatal Error: Unable to register with WSM. | The WAN board (the SYNC/570 driver specifically) was unable to register with the upper levels of the protocol stack. Check the board configuration.
SYNC570: PCI Adapter (Device ID = XXXX) -- revision must be 1 or greater. Adapter skipped. | Revision 0 of the SYNC/570ip boards cannot be used with this driver. You must have revision 1 or greater.
SYNC570: PCI Adapter has resource mapped above 1 Meg. Adapter skipped. | The current driver works with adapters running in legacy mode (i.e. all memory resources are mapped below 1 Megabyte.) Future versions will remove this restriction. The offending PCI adapter is not made available to the driver.
SYNC570: WARNING: Config File Not Found, Using Defaults. | Check the driver configuration and the load line that installs it.
SYNC570: WARNING: Config Record Error, Using Defaults.
SYNC570: WARNING: Maximum Packet Size smaller than Configured MRU Size using smaller value. | The Maximum internal packet size is smaller than the size configured. The lesser of the two values is being used.
SYNC570: Fatal Error: Bad Channel/Line No Param. | An invalid channel number has been selected. An example would be trying to install channel 3 of a 2 port board. Check your board installation.
SYNC570: Fatal Error: The board cannot be found at IO port. | The board does not appear to be at that IO port. Please check your dipswitch settings.
SYNC570: Fatal Error: The Board is already initialized. | The driver has been called twice for the same board and port combination.
SYNC570: Fatal Error: The board memory address conflicts with system memory. | The SYNC/570 has been configured to be at an already allocated memory address. Please select another address.
SYNC570: Fatal Error: Board RAM failed the memory test. | A memory test has been executed on the SYNC/570 and this test has failed. Please check that there are no other adapters trying to use the selected memory address. This may indicated board failure.
SYNC570: Fatal Error: Channel already in use. | The selected channel has already been configured.
SYNC570: Fatal Error: Config File Not Found, Exiting | The name= parameter of the board load line has not been configured. Ensure that the driver load line (ex. "load SYNC/570.LAN port=120 mem=d8000 int=5 channel=1 name=fred") is the same as the configured board.
SYNC570: Fatal Error: Duplicate Memory Address. | Another adapter has already registered the configured SYNC/570 memory address. Please select another.
SYNC570: Fatal Error: Incorrect Major or Minor Version Numbers. | The Major and Minor version numbers of the TSM are invalid. Check your MPR 3.1 installation.
SYNC570: Fatal Error: The initialization parameter is out of range | An attempt was made to initialize the board with a parameter that was invalid.
SYNC570: Fatal Error: The initialization parameter is in error. | An attempt was made to initialize the board with an incorrect parameter.
SYNC570: Fatal Error: Invalid PCI Board Number or Board not usable. | An adapter board number was specified that exceeds the number of PCI adapters the driver has detected and determined to be usable.
SYNC570: Fatal Error: Maximum Number of Boards exceeded. | The driver supports up to four SYNC/570 adapters and that limit has been exceeded.
SYNC570: Fatal Error: Memory for the board could not be allocated. | The driver was unable to allocated memory for internal functions.
SYNC570: Fatal Error: No Port Addr Param. | The port address was not included on the command line. Make sure a port=xxx parameter is included on the load line.
SYNC570: Fatal Error: A null pointer was passed as an initialization parameter | The board was unable to be initialized.
SYNC570: Fatal Error: Parse Driver Parameter. | Invalid parameters were selected on the load line. Please check the load line for accuracy.
SYNC570: Fatal Error: SNMP Registration Failed. | The SNMP support was unable to register.
SYNC570: Fatal Error: TSM Port Registered Error. | Registration with the TSM failed. Ensure that the TSM has loaded. Check the board configuration.
SYNC570: Fatal Error: Unable to get memory. | The driver was unable to allocate memory for internal usage.
SYNC570: Fatal Error: Unable to get resource tag. | The driver attempted to allocate a resource tag and failed.
SYNC570: Fatal Error: Unable to get TSM entries. | The driver was unable to get the TSM entry points. Check board and port configuration along with MPR installation.
SYNC570: Fatal Error: Unable to Initialize Board. | Board initialization failed. Run diagnostics on the board.
SYNC570: Fatal Error: Unable to Initialize Port. | Port Initialization failed. Check for a bad board. Check port configuration in INETCFG.
SYNC570: Fatal Error: Unable to register with WSM. | The WAN board (the SYNC/570 driver specifically) was unable to register with the upper levels of the protocol stack. Check the board configuration.
SYNC570: PCI Adapter (Device ID = XXXX) -- revision must be 1 or greater. Adapter skipped. | Revision 0 of the SYNC/570ip boards cannot be used with this driver. You must have revision 1 or greater.
SYNC570: PCI Adapter has resource mapped above 1 Meg. Adapter skipped. | The current driver works with adapters running in legacy mode (i.e. all memory resources are mapped below 1 Megabyte.) Future versions will remove this restriction. The offending PCI adapter is not made available to the driver.
SYNC570: WARNING: Config File Not Found, Using Defaults. | Check the driver configuration and the load line that installs it.
SYNC570: WARNING: Config Record Error, Using Defaults.
SYNC570: WARNING: Maximum Packet Size smaller than Configured MRU Size using smaller value. | The Maximum internal packet size is smaller than the size configured. The lesser of the two values is being used.