### Configuring a Device with pmadm

Use this procedure to enable and configure a Digi device with pmadm. This procedure can be used from a command line prompt in the absence of a window interface to the operating system. For additional information and help on pmadm, consult your Solaris documentation.

#### Procedure

1. Enter a pmadm command at a root prompt. Here is an example of a command that will enable a port for 9600 8,1,N. Modify the command as necessary for your terminal.
   `pmadm -a -p zsmon -s a001s -fu -i root -v `ttyadm -V`
   -m "`ttyadm -d /dev/term/a01s -l 9600 -s /usr/bin/login`"`
   where:

   zsmon | is the port monitor tag. Use a different one if appropriate.
   a001s | is the name of the device. Refer to your Digi manual for your device names.
   -l 9600 | sets the port for a baud rate of 9600.

2. Verify that the port is enabled with this command:

   `pmadm -l`