### Assigning an IP Address: DgIPserv

Use this procedure to store an IP address temporarily in an EtherLite module. The Digi BootP utility should work on any Microsoft Windows system.

#### Procedure

1. Download the DgIPserv utility file from the Digi website at http://support.digi.com. It is located in the sts_els folder under Diagnostic Utilities.
2. Connect the EtherLite module to the network.

   Note: Do not plug the power cable in to the EtherLite module.

3. Open the DgIPserv.exe program. The message "Watching for Bootp Requests" appears.
4. Choose File then Edit Bootp Response.
5. Enter the MAC address. The MAC address is found on the back panel next to the power outlet.

   Note: The first six digits or letters (00AOE7) are already entered. Enter only the last six letters and digits. Each EtherLite module needs a separate IP address.

6. Enter the IP address you want to assign the EtherLite module.
7. Plug in the power cable and a confirmation message should appear displaying the MAC Address and the new IP address.
8. Verify the network connection of the EtherLite module by using the Ping program. See Using Ping.