### Installing the Driver: CD

Use this procedure to install a driver from the Digi CD.
Note: The EtherLite module must have an IP address assigned before the driver is installed.

#### Procedure

1. Choose an operating system.
2. Choose a product.
3. Choose Install Software.
4. Follow the prompts. Enter the IP address when it is requested.
5. Reboot the system.
6. Verify the installation of the EtherLite module by selecting Control Panel > Ports. The new ports for the EtherLite module will be displayed.