### General SCO UnixWare Device Configuration

Use this information to configure serial ports, which includes configuring port direction (incoming and outgoing), transmission speed, and other port attributes.

Note: Users without SCO UnixWare should use the procedures found in General SVR4 Device Configuration.

1. Start the SCO Serial Manager by entering this command at a SCO UnixWare command prompt:

   `scoadmin serial`

2. Choose View and change the selection from Ports to Boards.
3. Choose the ncxa daemon for Digi RealPort.
4. Choose View and change from Boards to Ports. The ports will be listed.
5. Configure the ports as needed. Use the SCO UnixWare online help for additional information.
6. Exit the SCO Serial Manager.

Note: There is a bug in the SCO UnixWare Serial Manager that causes it to incorrectly set the "o" and "P" ttymon flags for a RealPort modem port. If the port does not work for logins, you may need to remove these flags. Use the `realport_pm_flags` program to list all non-console ttymon port monitor flags and change them appropriately.