### Creating Installation Diskettes: UNIX

Use this procedure to create a driver diskette from UNIX.

#### Procedure

Repeat these steps for each driver file.

1. Format a blank 1.44 megabyte floppy diskette in UNIX.

   Examples of Format Commands:

   Operating System | Format Command
   SCO Unix | format /dev/rfd0135ds18 (3-1/2 inch high density)
   SVR4 | format /dev/rdsk/f03ht (3-1/2 inch high density)
   Unix 3.2 | format /dev/rdsk/f03ht (3-1/2 inch high density)
   AIX | format /dev/fd0 (3-1/2 inch high density)

2. Access a root (su) prompt on the UNIX system.

3. Use a UNIX dd command to copy the driver to the formatted floppy.

   Generic Example:

   dd if=driver file of=floppy drive device bs=60k

   Note: Do not use the raw device with dd for floppy drive device (omit r from the device used in the format command in step 1).

   Specific Example:

   dd if=1019Z.bin of=/dev/fd0135ds18 bs=60k

   The dd command should copy the driver successfully to the diskette.