### Clearing a Busied-Out Channel

Use this procedure to clear a modem or B channel that previously has been busied out. That is, it enables the channel to handle traffic again.

1. Access the clearing function from the Line Summary screen.

Adapter | Screen
--- | ---
DataFire RAS 24/48 and DataFire DSP 24/48 | Line Summary screen
AccelePort RAS | Modem Summary screen

2. Choose the Clear option associated with the busied-out channel you want to clear.
3. At the prompt, choose OK.

> The Clear option will change to Busy Out and the State field will return to Idle on the Line Summary or Modem Summary screen. See Busying Out a Channel for more information about this function.