### Setting Up a Line with dgrascfg

Use this procedure to set up your Digi RAS adapter for provisioning of a line with the dgrascfg utility.

#### Procedure

1. At the command prompt, type the following: load dgrascfg.
2. Choose Configure/View Boards from the menu.
3. Highlight an adapter and press ENTER.
4. Set up each port (line) on the adapter. Keep the following in mind:
   - Choose the parameters that match the provisioning of the line. For more information about parameters, press F1 for online help.
   - Be sure to save the settings.
5. When configuration is complete, exit dgrascfg and then down and restart the server.