#### Information to Gather: Basic Rate ISDN (BRI) Configuration Worksheet

Use the form below to gather the information that may be required to complete the configuration of your DataFire RAS B4STU adapter within your operating system environment. Note that not all operating systems support all parameters.

With the exception of Modem Nationality, all parameters should be obtained from your service provider.

Parameter | Value
--- | ---
Switch Type | [ ] 5ESS [ ] DMS100 [ ] ETSI (Euro ISDN) [ ] INS-64 (Japan) [ ] NI1 [ ] None
Directory Number | List the telephone number of each logical terminal:
SPID or Subaddress | For switch types 5ESS, DMS100, NI1 and None, list the SPID (Service Profile Identifier) for each logical terminal; for switch types ETSI (Euro ISDN) and INS-64, list the Subaddress of each logical terminal:
Modem Nationality | Enter the country in which the RAS B4STU adapter will be installed:
MSN (Multiple Subscriber Numbers) | Available only for ETSI (Euro ISDN) switch type, in Linux installations. [ ] Disabled [ ] 1-8 (specify):
Leased Channels | List which, if any, B-channels are leased: