### Installing the Driver: Downloaded

Use one of the following procedures to install a downloaded SCO UnixWare driver. This procedure creates an installable driver diskette (or diskettes) readable by UNIX.

#### Procedures

##### Procedure 1: Installing from a Diskette with pkgadd

1. Download the appropriate driver file(s).
2. Create installation diskettes from the downloaded image files. This procedure is different, depending on the operating system you use to download the files and create the diskettes:

   Windows 3.x/95/98/DOS | Creating Installation Diskettes: Windows 3.x/95/98/DOS
   Windows 2000/NT | Creating Installation Diskettes: Windows NT and Windows 2000
   UNIX | Creating Installation Diskettes: UNIX

3. Log in as root on the UNIX system.
4. Insert the newly-created driver diskette.
5. Enter this command at a root prompt: pkgadd -d diskette1
6. Follow the system prompts to install the driver.

##### Procedure 2: Installing from a Diskette with SCO Admin

Note: This procedure must be done in an X Window environment.

1. Download the appropriate driver file(s).
2. Create installation diskettes from the downloaded image files. This procedure is different, depending on the operating system you use to download the files and create the diskettes:

   Windows 3.x/95/98/DOS | Creating Installation Diskettes: Windows 3.x/95/98/DOS
   Windows 2000/NT | Creating Installation Diskettes: Windows NT and Windows 2000
   UNIX | Creating Installation Diskettes: UNIX

3. Log in as root on the UNIX system.
4. Insert the newly-created driver diskette.
5. Select SCO Admin in the window environment or enter scoadmin at a root prompt.
6. Open the Software Management folder in the System Administration window.
7. Choose Application Installer.
8. Choose Disk_A from the Install from: menu.
9. Choose Update View.
10. Choose the Digi driver to install.
11. Choose Install.

12. Follow the system prompts to install the driver.