### Configuration Procedure

This topic describes how to configure the Digi device's SNMP agent.

#### Starting Point

This procedure assumes that you have logged on as the administrator and gather the following information:

- The IP address of the manager to which traps are sent
- The name and location of the SNMP contact person
- The SNMP name of the Digi device you are configuring

#### Procedure

Issue a set snmp command to configure the SNMP agent. Specify the following:

- The IP address of an SNMP management station to which traps are to be sent on the trap_dest field
- A name for this device on the snmp_name field
- A description of where the Digi device is located on the location field. If there are spaces in this entry, enclose it in quotation marks.
- The name of an SNMP contact person on the snmp_contact field. If there are spaces in this entry, enclose it in quotation marks.
- Whether authentication traps are generated when an authentication error occurs on the auth_trap field
- Whether the SNMP agent should run immediately on the run field

#### Configuration Example

`set snmp auth_trap=on trap_dest=190.174.150.10 location=Digi Minnesota snmp_name=blaze snmp_contact=bill jones run=on`