### RJ-45 8-Pin to Modem

The following table shows how to build a modem cable for EtherLite or SCSI Terminal Server, using an 8-pin RJ-45 plug.

##### RJ-45 Modem Cable

RJ-45 (Digi End) |  | DB-25 Male (Modem End)
--- | --- | ---
Signal | Pin | Pin | Signal
RTS | 1 | connected to | 4 | RTS
DSR | 2 | connected to | 6 | DSR
DCD | 3 | connected to | 8 | DCD
RxD | 4 | connected to | 3 | RxD
TxD | 5 | connected to | 2 | TxD
SG | 6 | connected to | 7 | SG
DTR | 7 | connected to | 20 | DTR
CTS | 8 | connected to | 5 | CTS