### Digi One RealPort and PortServer TS 2/4 Specifications

WARNING: To prevent electric shock, do not remove the cover of a Digi One RealPort or PortServer TS 2/4 module. There are no user-serviceable parts inside. Refer servicing to qualified personnel.

AC Power Requirements
1, 2 and 4-Port Units | 3.3 VDC ± 5%, 0.75 Amp (max) external power supply
Environmental
Ambient temperature | 50°F (10°C) to 122°F (50°C)
Relative humidity | 5% to 90% non-condensing
Altitude | 0 to 12,000 feet (0 to 3,658 meters)
Mechanical
Width Height Depth Weight | 6.9 inches (17.5 cm) 1 inch (2.5 cm) 3 inches (7.5 cm) pounds ( kg)