### Master Setup Process: X.25

Use this process to configure a SYNC 2000 line for X.25.

#### Procedure

1. Gather configuration information. See Information to Gather: X.25 Configuration.

2. Ensure that SCO patches have been installed. See Required SCO Patches.

3. Install the adapter. See the hardware installation card.

4. Install the Digi driver. See Installing the Driver: CD.

5. Add a WAN device. See Adding a WAN Device.

6. Configure a line for X.25. See Configuring a Line: X.25.