### ISDN E1 (Euro ISDN) Configuration Worksheet

Use the worksheet below to collect information that may be required to configure your DataFire PTE adapter in your operating system environment. Note that not all operating systems support all parameters.

The parameters on this page are for ISDN E1 (Euro ISDN).

Parameter | Value
--- | ---
Line Type | E1
Framing | [ ] CEPT with CRC4 [ ] CEPT without CRC4
Coding | [ ] HDB3
Signaling | [ ] ETSI (Euro ISDN) [ ] None
Modem Nationality | Enter the country in which the PTE adapter will be installed:
Switch Type | DSS1