### About dm_gui, dm_admin and dgdxb_config

#### Introduction

dm_gui, dm_admin and dgdxb_config are utilities which can be used to query and configure an AccelePort RAS adapter.

#### Uses for dm_gui

dm_gui is a graphical configuration and status utility. Note that dm_admin provides much of the same functionality in a command line user format. For information on using dm_gui, see Using dm_gui.

dm_gui may be used to:

- View adapter information such as adapter type, serial number, part number, and FEP version
- Reset ports
- View the status of port signals
- Display and change modem nationality

#### Uses for dm_admin

dm_admin is a command line configuration and status utility. Note that dm_gui provides much of the same functionality in a graphical user format. For information on using dm_admin, see Using dm_admin.

Among other things, dm_admin may be used to:

- Display and change modem nationality
- Display adapter information and status
- Query serial channel status and information

#### Uses for dgdxb_config

dgdxb_config is a utility used to view and change adapter information and to unload and reload adapters. For information on using dgdxb_config, see Using dgdxb_config.

dgdxb_config may be used to:

- View adapter information such as adapter type, serial number, adapter state and adapter designation letter
- Change the adapter designation letter
- Unload or Reload adapters

#### More Information

For more comprehensive information about the device driver and associated utilities, see the man pages for:

- dm_gui
- dm_admin
- dgdxb_config