### Configuring the Adapter: GUI

Use this procedure to access the dm_gui utility to view Digi RAS and AccelePort Xp adapter and port information, to reset ports, and to configure modem nationality (Digi RAS adapters only).

#### Configuration via the Dense Modem Control Panel

The Dense Modem Control Panel is a graphical utility, and requires an X Window System to be installed and running. If an X Window System is unavailable, the driver may be configured from the command line using dm_admin. See About dm_gui, dm_admin and dgdxb_config and Configuring the Adapter: Manual for details.

1. Log in as Super User (root).
2. Enter:

   `dm_gui

   ` The Dense Modem Control Panel appears.

3. Choose `Configure Adapter` (picture of adapter) or `Adapter Status` (picture of chart) to display or change settings. Use the online help for more information.

#### More Information

For more comprehensive information about dm_gui, see the man pages for dm_gui or use the dm_gui online help.