### Setting Ports to Auto-Answer

Use this procedure to set up a port for auto-answering. This procedure is required only if you want dial-in access.

#### Procedure

1. Create an entry in the Devices file:
   1. Navigate to the correct directory:

      `cd /etc/uucp`

   2. Display the directory contents:

      `ls`

   3. Open the Devices file with vi:

      `vi Devices`

   4. Navigate to the bottom of the file:

      `G`

   5. Open a new line:

      `0`

   6. Add an entry to the Devices list. Type:

      `Direct term/dg0async1s -9600 direct`

      and press ESC.

   7. Repeat for every port that you want to be able to auto-answer.
   8. Exit the vi editor:

      `ZZ`.

2. Enter `cu -l term/dg0async1s`.
3. To set a port to auto-answer, enter `ats0=1&w`.

   The system responds OK.

4. To view settings, enter `A+&v`.
5. Repeat these steps for each device that will be used for dial-in.
6. To exit, press `~` (tilde).