12-hour
Command Reference: set time
1st_ip_addr
Command Reference: set ippool
24-hour
Command Reference: set time
Abbreviating Commands
About the Command Line Interface
Abort Output
Command Reference: send
Abort Output: PortServer
Command Reference: set logins
Add Syntax
Command Reference: set telnet
Add Syntax: Line Feed Characters
Command Reference: mode
Address Resolution Protocol
Command Reference: set arp
Command Reference: set trace
Admin
Command Reference: admin
Administrative Terminal
Command Reference: cpconf
Aixon
Command Reference: set flow
Altip command
Command Reference: set altip
Altip command: Displaying
Command Reference: set altip
Altpin
Command Reference: set flow
Annexa
Command Reference: set framerelay
Annexd
Command Reference: set framerelay
Annexd MTU
Command Reference: set framerelay
Are You There
Command Reference: send
Arp
Command Reference: info
Arp range
Command Reference: set arp
ARP Table
Command Reference: set arp
ARP to route
Command Reference: set forwarding
ARP to route: route
Command Reference: set forwarding
ARP to route: tracing
Command Reference: set trace
ARP to route: view
Command Reference: set arp
Async status
Command Reference: info
Async status: Displaying
Command Reference: set port
Auth
Command Reference: set auth
Auth command
Command Reference: set auth
Auth Table
Command Reference: set auth
Auth_trap
Command Reference: set snmp
Auth_trap: Configuring
Command Reference: set port
Autoconnect ports
Command Reference: set port
Autoconnect ports: Configuring
Command Reference: set users
AutoHost
Command Reference: set users
AutoPort
Command Reference: set users
AutoService
Command Reference: set users
Ayt
Command Reference: send
Backoff timeout
Command Reference: set tcp
Baud
Command Reference: set device
Command Reference: set line
Baud: Configuring
Command Reference: set line
BcMax
Command Reference: set frdlci
BcMin
Command Reference: set frdlci
BECN
Command Reference: set framerelay
Binary Mode On
Command Reference: mode
Boot
Command Reference: boot
Command Reference: set config
Boot Host
Command Reference: boot
Bps
Command Reference: set device
Break
Command Reference: send
Command Reference: set config
Bringup
Command Reference: set filter
Command Reference: set users
Brk
Command Reference: send
Bypass the PortServer’s login
Command Reference: set port
Bypass the PortServer’s login: Key
Command Reference: set keys
Bypass the PortServer’s login: Password
Command Reference: newpass
CHAP
Command Reference: set users
Chat Table
Command Reference: set device
Chat Table: Configuring
Command Reference: set chat
Chat Table: Displaying
Command Reference: set chat
Chat Table: Renaming
Command Reference: set chat
Chat_name
Command Reference: set chat
Chatname
Command Reference: set chat
CIR
Command Reference: set frdlci
Clear All Network Statistics Tables
Command Reference: info
Close
Command Reference: close
Closes a WAN
Command Reference: wan
Closes a WAN: WAN
Command Reference: wan
Closes a WAN: WAN Interface
Command Reference: wan
Clrseq
Command Reference: set terms
Command Line Interface
About the Command Line Interface
Command Line Interface: Abbreviating
About the Command Line Interface
Config
Command Reference: set config
Configure Unlimited Access to a Port
Command Reference: set auth
Configuring
Command Reference: set line
Configuring: Autoconnect
Command Reference: set port
Configuring: Baud
Command Reference: set line
Configuring: Device
Command Reference: set device
Configuring: Entry
Command Reference: set service
Configuring: Flow Control Settings
Command Reference: set flow
Configuring: keep-alive Parameters
Command Reference: set tcp
Configuring: Login Script
Command Reference: set script
Configuring: Mixed Access
Command Reference: set auth
Configuring: Name-to-IP Address Mapping
Command Reference: set host
Configuring: Port
Command Reference: set framerelay
Configuring: PortServer
Command Reference: set host
Configuring: Primary RADIUS Server
Command Reference: set radius
Configuring: Proxy ARP
Command Reference: set forwarding
Configuring: Route
Command Reference: set route
Configuring: TCP Maximum Retransmission Timeout Value
Command Reference: set tcp
Configuring: TCP Socket Service
Command Reference: set tcp
Configuring: Terminal Type
Command Reference: set terms
Configuring: Trace Levels
Command Reference: set trace
Configuring: Two RADIUS Servers
Command Reference: set radius
Configuring: Virtual Circuit
Command Reference: set frdlci
Connect
Command Reference: connect
Command Reference: set port
Command Reference: set users
ConnectEsc
Command Reference: close
Command Reference: set users
Connection
Command Reference: set port
Connection: From
Command Reference: cpconf
Connection: Initiating
Command Reference: connect
Connection: reattempting
Command Reference: set users
Connection: RST
Command Reference: info
Connection: To
Command Reference: cpconf
Cpconf
Command Reference: cpconf
Cpconf: Menu
Command Reference: set menu
Cpconf: Rules
Command Reference: set filter
Crlf
Command Reference: mode
Crmod
Command Reference: mode
CSLIP
Command Reference: set filter
Command Reference: set terms
Command Reference: set users
Command Reference: wan
Cts
Command Reference: set flow
Cts_sigchange
Command Reference: info
Current Port
Command Reference: set port
Datagram
Command Reference: info
Command Reference: set route
Command Reference: set trace
Datagram: Incoming
Command Reference: info
Datagram: Outgoing
Command Reference: info
Dcd
Command Reference: set flow
Dcd: Configuring
Command Reference: set device
Dcd: Displaying
Command Reference: set device
Dcd: Script
Command Reference: set script
Dcd: Virtual Circuit
Command Reference: set frdlci
DHCP
Command Reference: set trace
Dhcp command
Command Reference: set dhcp
Dhcp command: Enabling
Command Reference: set dhcp
Displaying
Command Reference: display
Command Reference: set line
Displaying: Altip Table
Command Reference: set altip
Displaying: Attributes
Command Reference: set port
Displaying: Complete Table
Command Reference: set config
Displaying: Current Port’s Scripts
Command Reference: set modem
Displaying: Device Table
Command Reference: set device
Displaying: Entire Auth Table
Command Reference: set auth
Displaying: Entire Chat Table
Command Reference: set chat
Displaying: Entire Term Table
Command Reference: set terms
Displaying: Entire User Table
Command Reference: set users
Displaying: Entry
Command Reference: set framerelay
Command Reference: set host
Command Reference: set script
Displaying: Filter Stanzas
Command Reference: set filter
Displaying: Filter Table
Command Reference: set filter
Displaying: Flow Control Settings
Command Reference: set flow
Displaying: Frame Relay Table
Command Reference: set framerelay
Displaying: Host Table
Command Reference: set host
Displaying: IP Routing Table
Command Reference: set forwarding
Displaying: IP Table
Command Reference: info
Displaying: Key Table
Command Reference: set keys
Displaying: Login Information
Command Reference: set logins
Displaying: Menu Table
Command Reference: set menu
Displaying: Operating Parameters
Command Reference: mode
Displaying: port’s
Command Reference: set port
Displaying: RADIUS Configuration
Command Reference: set radius
Displaying: Range
Command Reference: set route
Displaying: Route Table
Command Reference: set route
Displaying: Script Table
Command Reference: set script
Displaying: Serial Line Parameters
Command Reference: set line
Displaying: Service Table
Command Reference: set service
Displaying: SNMP Configuration
Command Reference: set snmp
Displaying: Time
Command Reference: set time
Displaying: Trace Settings
Command Reference: set trace
Displaying: Virtual Circuit Parameters
Command Reference: set frdlci
Displaying: WAN Status Information
Command Reference: wan
Dlci
Command Reference: set frdlci
DLCIs
Command Reference: info
Command Reference: set users
DNS
Command Reference: set host
Command Reference: set trace
Command Reference: telnet
DNS name
Command Reference: traceroute
Domain Name System
Command Reference: set trace
DownDly
Command Reference: set users
Dsr
Command Reference: set flow
Dst
Command Reference: set filter
Dtr
Command Reference: set flow
Dynamic Host Configuration Protocol
Command Reference: set config
Command Reference: set dhcp
Edelay
Command Reference: set ports
Edelay: increasing
Command Reference: set ports
Editing Keys
About the Command Line Interface
Eewrite
Command Reference: boot
Eewrite: DHCP
Command Reference: set config
Command Reference: set dhcp
Eewrite: keep-alive
Command Reference: set tcp
Erase Character
Command Reference: send
Erase Line
Command Reference: send
Escape
Command Reference: send
Escape sequence
Command Reference: set terms
Ethernet
Command Reference: set config
Ethernet: ARP table contains
Command Reference: set arp
Exit
Command Reference: exit
Exit: Displaying
Command Reference: set filter
Exit: Displaying
Command Reference: set filter
Exit: Removing
Command Reference: set filter
Exit: Source IP Address
Command Reference: set filter
Filter-ppp01
Command Reference: wan
Filter-ppp01: Configuring
Command Reference: set flow
Filter-ppp01: Displaying
Command Reference: set flow
Filter-ppp01: proxyarp
Command Reference: set forwarding
Frame Relay
Command Reference: info
Command Reference: set framerelay
Command Reference: set frdlci
Frame Relay: Displaying
Command Reference: set framerelay
Frdlci
Command Reference: set frdlci
Fromhost
Command Reference: cpconf
Fromhost: SNMP OID
Command Reference: set snmp
Go Ahead
Command Reference: send
Go Ahead: Displaying
Command Reference: set host
Host_name
Command Reference: set host
Host_name ip
Command Reference: set host
Hr.min.sec
Command Reference: set time
Hrmode
Command Reference: set time
Hunt_group
Command Reference: connect
ICMP
Command Reference: info
Command Reference: ping
Command Reference: set config
ICMP routing
Command Reference: set config
ICMP routing: Connection
Command Reference: connect
ICMP routing: datagrams
Command Reference: info
Initmodem
Command Reference: wan
Interface_table
Command Reference: info
Internet Control Message Protocol
Command Reference: set trace
Interrupt Process
Command Reference: send
Interrupt Process: command displays
Command Reference: info
Interrupt Process: names
Command Reference: set host
Interrupt Process: processing
Command Reference: info
Interrupt Process: Renew
Command Reference: set dhcp
IP Address
Command Reference: set ippool
IP Address: Displaying
Command Reference: set forwarding
IP Address: Removing
Command Reference: set altip
IP Address: route
Command Reference: set altip
IP Statistics
Command Reference: info
IP Statistics: Displaying
Command Reference: info
IP Time To Live
Command Reference: set tcp
Ip_addr
Command Reference: set host
Ip_ttl
Command Reference: set tcp
Ippool command
Command Reference: set ippool
Itoss
Command Reference: set flow
Ixany
Command Reference: set flow
Ixoff
Command Reference: set flow
Ixon
Command Reference: set flow
Ixon: Configuring
Command Reference: set tcp
Ixon: disable
Command Reference: set tcp
Ixon: enable
Command Reference: set tcp
Ixon: Set
Command Reference: set tcp
Ixon: telnet session enables
Command Reference: set tcp
Keepup
Command Reference: set filter
Command Reference: set users
Keepup: Adding
Command Reference: mode
Keepup: Changing
Command Reference: set keys
Keepup: command changes
Command Reference: set keys
Keepup: Displaying
Command Reference: set keys
Keepup: TTY Session
Command Reference: kill
LMI
Command Reference: info
Command Reference: set framerelay
Lmirev1
Command Reference: set framerelay
Login
Command Reference: set logins
Command Reference: set port
Command Reference: set script
Login: Displaying
Command Reference: set logins
Logins command
Command Reference: set logins
Loginscript
Command Reference: set script
Logpacket
Command Reference: set filter
Loose Source Routing
Command Reference: ping
Loose_sroute
Command Reference: ping
Loose_sroute: Creating
Command Reference: set menu
Loose_sroute: Display Lines
Command Reference: set menu
Loose_sroute: Displaying
Command Reference: set menu
Loose_sroute: Removing
Command Reference: set menu
Mixed Access
Command Reference: set auth
Mon.day.yr
Command Reference: set time
MTU
Command Reference: set framerelay
Multiscreen
Command Reference: set port
Multisession
Command Reference: set port
Multisession: Configuring
Command Reference: set host
Multisession: IP
Command Reference: set host
Net_addr
Command Reference: set route
NetService
Command Reference: set users
Network Statistics
Command Reference: info
Network Statistics: enter
Command Reference: newpass
NN1
Command Reference: set framerelay
NN2
Command Reference: set framerelay
NN3
Command Reference: set framerelay
No Operation
Command Reference: send
Nop
Command Reference: send
NT1
Command Reference: set framerelay
NT1: Telnet Session
Command Reference: telnet
Overruns
Command Reference: info
Parity
Command Reference: set line
Poisonreverse
Command Reference: set forwarding
Poisonreverse: Configuring
Command Reference: set ippool
Poisonreverse: Removing
Command Reference: set ippool
Port
Command Reference: set auth
Command Reference: set port
Port ids
Command Reference: set port
Port ids: Configure Unlimited Access
Command Reference: set auth
Port ids: Configuring
Command Reference: set framerelay
PPP
Command Reference: set filter
Command Reference: set users
Command Reference: wan
PPP: Configuring
Command Reference: set radius
Probe_cnt
Command Reference: set tcp
Probe_count
Command Reference: set tcp
Probe_interval
Command Reference: set tcp
Protocol_table
Command Reference: info
ProtoEncap
Command Reference: set frdlci
ProtoEncap: Configuring
Command Reference: set forwarding
Quit
Command Reference: quit
RADIUS
Command Reference: set trace
RADIUS: Displaying
Command Reference: set route
RADIUS: Displaying
Command Reference: set radius
RADIUS: searching
Command Reference: set radius
RARP
Command Reference: set config
Rcv
Command Reference: set filter
Rcv: port number
Command Reference: set config
RealPort connections
Command Reference: set config
Reboot Syntax
Command Reference: boot
Command Reference: kill
Reconnect
Command Reference: reconnect
Removing
Command Reference: set terms
Removing: Chat Table Entry
Command Reference: set chat
Removing: Chat Table Entry
Command Reference: set chat
Removing: Entry
Command Reference: set route
Command Reference: set terms
Removing: Filter
Command Reference: set filter
Removing: IP
Command Reference: set dhcp
Removing: IP Address
Command Reference: set altip
Removing: Pool
Command Reference: set ippool
Removing: PortServer
Command Reference: boot
Removing: User
Command Reference: set users
Restore
Command Reference: cpconf
Restore Configuration Defaults
Command Reference: boot
Restore Configuration Defaults: PortServer
Command Reference: boot
Retransmission
Command Reference: set tcp
Retransmission timeout
Command Reference: set tcp
Retransmission timeout: number
Command Reference: set frdlci
Reverse Address Resolution Protocol
Command Reference: set config
RFC 1490
Command Reference: set frdlci
Ri
Command Reference: set flow
RIP
Command Reference: set config
Command Reference: set route
Command Reference: set users
Rlogin
Command Reference: set users
Rlogin: Enter
Command Reference: rlogin
RLoginEsc
Command Reference: close
Command Reference: set users
Rmarp
Command Reference: set arp
Rmauth
Command Reference: set auth
Rmchat
Command Reference: set chat
Rmdevice
Command Reference: set device
Rmfilter
Command Reference: set filter
Rmhost
Command Reference: set host
Rmroute
Command Reference: set route
Rmroute: ARP
Command Reference: set forwarding
Rmroute: Configuring
Command Reference: set route
Rmroute: Displaying
Command Reference: set route
Routing Information Protocol
Command Reference: set forwarding
Rto_max
Command Reference: set tcp
Rts
Command Reference: set flow
Script
Command Reference: set modem
Command Reference: set script
Script: Abort Output
Command Reference: send
Script: Are You There
Command Reference: send
Script: Break
Command Reference: send
Script: Delete
Command Reference: set script
Script: Displaying
Command Reference: set script
Script: Erase Character
Command Reference: send
Script: Erase Line
Command Reference: send
Script: Escape
Command Reference: send
Script: Go Ahead
Command Reference: send
Script: Interrupt Process
Command Reference: send
Script: No Operation
Command Reference: send
Script: Synchronize Process
Command Reference: send
Send AYT
Command Reference: send
Send IP
Command Reference: send
Send IP: Displaying
Command Reference: set line
Serial Statistics
Command Reference: info
Serial Statistics: Displaying
Command Reference: set service
Servicename
Command Reference: set filter
Session
Command Reference: info
Set altip
Command Reference: set altip
Set arp
Command Reference: set arp
Set auth
Command Reference: set auth
Set chat
Command Reference: set chat
Set config
Command Reference: set config
Set device
Command Reference: set device
Set dhcp
Command Reference: set dhcp
Set filter
Command Reference: set filter
Set flow
Command Reference: set flow
Set framerelay
Command Reference: set framerelay
Set frdlci
Command Reference: set frdlci
Set host
Command Reference: set host
Set ippool
Command Reference: set ippool
Set keys
Command Reference: set keys
Set line
Command Reference: set line
Set logins
Command Reference: set logins
Set menu
Command Reference: set menu
Set modem
Command Reference: set modem
Set ports
Command Reference: set port
Set radius
Command Reference: set radius
Set route
Command Reference: set route
Set script
Command Reference: set script
Set service
Command Reference: set service
Set snmp
Command Reference: set snmp
Set tcp
Command Reference: set tcp
Set telnet
Command Reference: set telnet
Set terms
Command Reference: set terms
Set time
Command Reference: set time
Set trace
Command Reference: set trace
Set users
Command Reference: set users
Set_request
Command Reference: set snmp
Set_request: keepalive_idle
Command Reference: set tcp
Set_request: SNMP OID
Command Reference: set snmp
Set_request: tcp realport
Command Reference: set tcp
Set_request: Time
Command Reference: set time
Simple Network Management Protocol
Command Reference: set snmp
Command Reference: set trace
SLIP
Command Reference: set filter
Command Reference: set users
Command Reference: wan
Snmp
Command Reference: set snmp
Command Reference: set trace
SNMP daemon
Command Reference: set snmp
SNMP daemon: Displaying
Command Reference: set snmp
SNMP daemon: Filtering
Command Reference: set filter
SNMP daemon: getting
Command Reference: set snmp
SNMP daemon: setting
Command Reference: set snmp
Splithorizon
Command Reference: set forwarding
Src
Command Reference: set filter
Sroute
Command Reference: ping
Stanzas
Command Reference: set script
Start-up
Command Reference: wan
Start-up: WAN Interface
Command Reference: wan
Status
Command Reference: info
Command Reference: status
Stop Bits
Command Reference: set line
Strict Source Routing
Command Reference: ping
Strict_sroute
Command Reference: ping
Subnet
Command Reference: set config
Superuser
Command Reference: admin
Synchronize Process
Command Reference: send
Tbreak
Command Reference: set config
TCP
Command Reference: set config
TCP connections
Command Reference: info
Tcp keepalive_idle
Command Reference: set tcp
TCP Maximum Retransmission Timeout Value
Command Reference: set tcp
TCP Maximum Retransmission Timeout Value: Set
Command Reference: set tcp
TCP Socket Service
Command Reference: set tcp
TCP Statistics
Command Reference: info
Telnet
Command Reference: set telnet
Command Reference: set users
Command Reference: telnet
Command Reference: mode
Telnet operating
Command Reference: mode
Telnet Session
Command Reference: mode
Telnet Session: Opening
Command Reference: telnet
TelnetEsc
Command Reference: close
Command Reference: set users
Term Table
Command Reference: set terms
Terminal Type
Command Reference: set terms
Terminal Type: Configuring
Command Reference: set terms
Termtype
Command Reference: set terms
Testmodem
Command Reference: wan
Testmodem: Changing
Command Reference: set arp
Testmodem: Displaying
Command Reference: set time
Testmodem: Setting
Command Reference: set time
Time To Live
Command Reference: set tcp
Tohost
Command Reference: cpconf
Tohost: Configuring
Command Reference: set trace
Tohost: Displaying
Command Reference: set trace
Traceroute
Command Reference: traceroute
Traceroute command
Command Reference: traceroute
Traceroute command: ARP
Command Reference: set trace
Traceroute command: Enter
Command Reference: traceroute
Traceroute command: Use
Command Reference: traceroute
Trap
Command Reference: set snmp
Trap_dest
Command Reference: set snmp
Trap_dest: Killing
Command Reference: kill
UDP command
Command Reference: info
UDP datagrams
Command Reference: info
UDP port
Command Reference: set filter
UDP Statistics
Command Reference: info
UDP Statistics: rmauth
Command Reference: set auth
User
Command Reference: who
User Configuration
Command Reference: set logins
User Table
Command Reference: set users
User Table: Removing
Command Reference: set users
Username
Command Reference: newpass
Username: ARP
Command Reference: set arp
Username: closes
Command Reference: wan
Username: Configuring
Command Reference: set frdlci
Username: Deleting
Command Reference: set frdlci
Username: Displaying
Command Reference: wan
Username: Displaying
Command Reference: set frdlci
Username: initiates
Command Reference: wan
Username: uses
Command Reference: set route
WAN Connection
Command Reference: set route
WAN Connection: Closing
Command Reference: wan
WAN Connection: Displaying
Command Reference: wan
WAN Connection: Starting
Command Reference: wan
Wanname
Command Reference: set route
Command Reference: wan