### Configuring an IP Address with RARP

Use this topic to configure the Digi One RealPort or PortServer TS IP address from a RARP server. Digi devices will send out a RARP request for an address only if they have not been assigned one already.

#### Starting Point

This procedure assumes that the Digi device is connected to the Ethernet network.

#### Procedure

1. Set up RARP tables as required on your RARP server.
2. Turn the Digi device on.

An IP address is automatically assigned.