### PortServer TS 8/16 Specifications

WARNING: To prevent electric shock, do not remove the cover of a PortServer TS 8/16 module. There are no user-serviceable parts inside. Refer servicing to qualified personnel.

AC Power Requirements
16-Port Desktop, 16-Port Rack | 90-264 VAC, 47-63 Hz, .6 Amp (max) internal power supply
8-Port Desktop | 12 VDC, .4 Amp (max) external power supply
Environmental
Ambient temperature | 60°F (15.6°C) to 90°F (32.2°C)
Relative humidity | 20% to 80% non-condensing
Altitude | 0 to 7,000 feet (0 to 2,134 meters)
Mechanical
16-Port Rack | Width: 16.8 inches (42.672 cm) Height: 1.6 inches (4.064 cm) Depth: 6.5 inches (16.510 cm) Weight: 3.75 pounds (1.701 kg)
16-Port Desktop | Width: 13.5 inches (34.290 cm) Height: 1.375 inches (3.493 cm) Depth: 6.5 inches (16.510 cm) Weight: 3 pounds (1.360 kg)
8-Port Desktop | Width: 8.25 inches (20.955 cm) Height: 1.125 inches (2.858 cm) Depth: 3.75 inches (9.526 cm) Weight: 1.21 pounds (0.549 kg)