### Device Names

The devices will be created in /dev/dg/dgdm, linked to /dev, and will have the following format:

Dial-in devices: ttyGa_xx, where a is the adapter number and xx is the device number.

Dial-out devices: cuga_xx, where a is the adapter number and xx is the device number.

DigiPRINT transparent printer devices: lpGa_xx, where a is the adapter number and xx is the device number.

Device and adapter numbers start at zero.

#### Example:

Port 4 of Adapter 3 is /dev/cug2_03. The same port with modem control is /dev/ttyG2_03. The DigiPRINT device is /dev/lpG2_03.