### DataFire PTE Configuration Worksheet

#### ISDN T1 (PRI), Long Haul (External T1)

Use the worksheet below to collect the information that may be required to complete the configuration of your DataFire PTE adapter within your operating system environment. Note that not all operating systems support all parameters.

The parameters on this page are for ISDN T1 (PRI) connected directly to an external T1 telephone line (Long Haul). If your adapter is connected to a PBX or similar in-house network, use the ISDN T1 (PRI), Short Haul (PBX or Other Internal Network) configuration worksheet.

Parameter | Value
--- | ---
Coding | [ ] B8ZS
Framing | [ ] ESF
Long Haul Line Build Out (Level) | [ ] 0dB [ ] 7.5 dB [ ] 15 dB [ ] 22.5 dB
Signaling | [ ] AT&T 5ESS [ ] Nortel DMS 100/250 [ ] ETSI (Euro ISDN) [ ] INS-1500 (Japan) [ ] National ISDN2 [ ] None
NFAS Master Port (RAS 48 PT2 Only) | [ ] None [ ] 1 [ ] 2 | Interface ID for Port 1 (0-127): ________ | Interface ID for Port 2 (0-127): ________
Leased Time Slots | List which, if any, PRI time slots are leased:
Modem Nationality | Enter the country in which the PTE adapter will be installed: