### DataFire SYNC/570 Specifications

Power Requirements
SYNC/570 | 750mA @ +5 VDC
40mA @ ± 12 VDC
SYNC/570 PCI UIB | 1.5A @ +5V DC
50mA @ ± 12 V
Temperature | 10º to 55º C (50º to 131ºF)
Relative Humidity | 5% to 90%, non-condensing
Air Movement | 30 CFM Forced
Altitude | 0 to 3658 meters (12000 ft.)
USART | Hitachi HD64570 Serial Communications Adapter 10Mhz
Memory | 128KB Dual-Ported (tri-stated)
Shared Memory Window | 16KB (assignable within first 16MB of system memory)
Serial Ports | Two EIA-232-D
Cabling | Two DB-15 (male) to DB-25 (male) 8 ft. cables
EIA-232-D Modem Signals | TxD, RxD, CTS, RTS, DSR, DTR, TxC, RxC, DCD
Connectors | Two DB-15 Female (High Density)
Baud Rate | Up to 5MB/second each line
DMA | Four channels (Hitachi HD64570)
Programmable Timers | Hitachi HD64570
I/O Address | ISA - hardware switch configurable
PC Interrupts | 3, 5, 7, 10, 12, 15 (software configurable)
SurgeBlock | Optional