### Installing the Driver: Downloaded

Use this procedure to install a downloaded Digi SVR4 UNIX or SCO UnixWare driver.

#### Procedure 1: Using pkgadd

1. Download the appropriate driver file(s).
2. Log in as root on the UNIX system.
3. Enter this command at a root prompt: pkgadd -d /path/filename

   where path is the path to the driver file and filename is the name of the driver file.

4. Follow the system prompts to install the driver.

#### Procedure 2: Using SCO Admin (SCO UnixWare)

Note: This procedure must be done in an X Window environment.

1. Download the appropriate driver file(s).
2. Create installation diskettes from the downloaded image files. This procedure is different, depending on the operating system you use to download the files and create the diskettes:

   Windows 3.x/95/98/DOS | Creating Installation Diskettes: Windows 3.x/95/98/DOS
   Windows 2000/NT | Creating Installation Diskettes: Windows NT and Windows 2000
   UNIX | Creating Installation Diskettes: UNIX

3. Log in as root on the UNIX system.
4. Insert the newly-created driver diskette.
5. Select <SCO Admin> in the window environment or type scoadmin at a root prompt.
6. Double-click the Software Management folder in the System Administration window.
7. Double-click <Application Installer>.
8. Choose <Disk_A> from the Install from: menu.
9. Choose <Update View>.
10. Choose the Digi driver to install.
11. Choose <Install>.

12. Follow the system prompts to install the driver.